BroadCaster Composer PRO-XL
Professional Audio Processing for Radio, Streaming and Broadcast
BroadCaster Composer PRO-XL is a highly precise virtual rack audio processor designed to make your broadcast audio sound professional, leveled, powerful and perfectly equalized.
It can be used as a standalone Windows application or as a VST3 plugin inside your playout, broadcasting or production software (DAW).
It is ideal for Internet radio, FM broadcasting, streaming, studio production, voiceover and professional music playout.

Professional Processing in One Virtual Rack
BroadCaster Composer PRO-XL combines several essential audio processors into one clear and efficient processing chain:
Input AGC → 10-Band EQ → Multiband Compressor → Peak Limiter
The result is more consistent volume, controlled dynamics, an optimized frequency response and a powerful broadcast sound.
Input AGC – Automatic Gain Control
The built-in Automatic Gain Control (AGC) helps maintain a consistent input level even when the volume of individual audio sources varies.
The following parameters can be adjusted:
· Target Level (dB) – desired average output level
· Speed (ms) – response speed to changes in volume
AGC is particularly useful for Internet radio broadcasting, where it helps smoothly balance differences between quieter and louder tracks.

10-Band Graphic Equalizer
Shape the character of your broadcast sound using the integrated 10-band graphic equalizer.
The equalizer operates across the range:
31 Hz – 16 kHz
Each band provides:
±15 dB of adjustment
This allows you to precisely shape bass, midrange and high frequencies and adapt the sound to your particular broadcasting style.
For example, low frequencies can be slightly boosted for a fuller bass response, while higher frequencies can be enhanced to provide greater clarity and presence for vocals.

Multiband Compressor
The integrated Multiband Compressor reduces the dynamic range and helps create a denser, more consistent and more powerful sound.
The available parameters include:
· Threshold (dB) – level at which compression begins
· Ratio – compression ratio
· Attack (ms) – compressor response time
· Release (ms) – compressor recovery time
This allows the processing to be adapted for both music broadcasting and spoken-word content.

Peak Limiter
At the end of the entire processing chain is the Peak Limiter.
Its purpose is to prevent the digital signal from exceeding the maximum level of 0 dBFS, helping protect the output from digital clipping.

Designed for Radio, Internet Broadcasting and Production
BroadCaster Composer PRO-XL is designed for a wide range of professional audio applications.
FM Radio / Internet Broadcast
For a modern, powerful and punchy broadcast sound, you can use more aggressive compression together with a so-called “smile” EQ curve, enhancing the low and high frequencies.
Speech / Voiceover
For clear and intelligible speech, unwanted low-frequency rumble can be reduced while the 1–4 kHz presence range can be slightly enhanced.
Moderate compression helps keep the voice upfront without making it sound unnecessarily artificial.

Standalone or VST3
Windows Standalone
Composer PRO-XL can be operated as a standalone application on Windows.
For the lowest possible latency, an ASIO-compatible audio interface is recommended. Windows WASAPI is also supported.
VST3 Plugin
Composer PRO-XL can also be used as a standard VST3 plugin inside compatible DAW, playout or broadcasting software.
The manual lists examples including:
· vMix
· OBS Studio
· Reaper
· Cubase
· Ableton
· FL Studio
· Radio Profesional
· RPX

Choose the License That Fits Your Needs
BroadCaster Composer PRO-XL is available in four license versions:
	Version
	Validity

	LIGHT
	1 year

	NORMAL
	2 years

	DELUXE
	5 years

	FOREVER
	Lifetime


Every license includes:
· Free lifetime updates
· Free lifetime upgrades
· Up to 5 activations
The license may be activated repeatedly on the same PC when reinstalling the operating system, or within a single entity – an individual or company – on up to 5 devices simultaneously.
This does not constitute a violation of the license terms.
Complete license terms:
urlLicense Terms – Licence.txthttps://download.mysoft.cz/Licence.txt

DOWNLOADS
The BroadCaster Composer PRO-XL software is available as a Windows standalone application and as a VST3 plugin.
Windows Application
Download the application here:
urlDownload BroadCaster Composer PRO-XL – Windows Applicationhttps://download.mysoft.cz/radioprocessor/RadioProcessor.exe
VST3 Plugin
Download the VST3 plugin here:
urlDownload BroadCaster Composer PRO-XL – VST3 Pluginhttps://download.mysoft.cz/radioprocessor/RadioProcessor.vst3

Manual & Documentation
Before installing or purchasing a license, you can review the complete product documentation.
English User Manual
Download the detailed English user manual:
urlDownload English User Manual – PDFhttps://download.mysoft.cz/radioprocessor/BroadCaster_Composer_PRO-XL_Manual.pdf
Czech User Manual
Download the Czech manual and detailed product description:
urlDownload Czech User Manual – PDFhttps://download.mysoft.cz/radioprocessor/BroadCaster_Composer_PRO-XL_Manual_CZ.pdf

License Activation
License activation is simple and is performed directly inside the application.
1. Open ABOUT or SETTINGS.
1. Copy your unique Instance ID.
1. Click Order License (Online) to proceed with your license purchase.
1. Once you receive your license key by e-mail, click Enter License Key.
1. Enter the license key and click Activate.
The application will verify the license online and unlock all product features.
After the initial activation, the software supports offline license verification, so a permanent Internet connection is not required for normal operation.
If no valid license is entered, the application operates in 1-hour Demo mode. After the demo period expires, audio processing is switched to Bypass mode.

Key Features
· Professional virtual rack audio processor
· Windows standalone application
· VST3 plugin
· Input AGC for automatic level control
· 10-band graphic EQ
· EQ frequency range 31 Hz – 16 kHz
· EQ adjustment range ±15 dB
· Multiband Compressor
· Threshold, Ratio, Attack and Release controls
· Peak Limiter
· Maximum digital level protection at 0 dBFS
· Designed for FM and Internet broadcasting
· Suitable for music and speech processing
· ASIO support
· Windows WASAPI support
· VST3 compatibility
· Offline license verification after initial activation
· Free lifetime updates
· Free lifetime upgrades
· Up to 5 license activations

System Requirements
Operating System
· Windows 10 64-bit
· Windows 11
Processor
· Intel Core i5 / AMD Ryzen 5 or newer
· AVX instruction support recommended for efficient DSP processing
Memory
· Minimum: 4 GB RAM
· Recommended: 8 GB RAM or more
Storage
· 50 MB of free disk space
Audio Interface
For the standalone version, an ASIO-compatible audio interface is recommended for the lowest possible latency.
Windows WASAPI is also supported.
VST3
Using the VST3 plugin requires a compatible DAW, playout or broadcasting application with VST3 support.

BroadCaster Composer PRO-XL
Professional audio processing for modern broadcasting.
AGC • 10-Band EQ • Multiband Compressor • Peak Limiter
Standalone + VST3 | Windows 10/11 | Up to 5 Activations | Free Lifetime Updates & Upgrades
